**Wall clock JVD N12010**

Instruction manual

1. Insert one “AA“ (1.5V) battery as indicated in the battery holder. The movement would be damaged if the battery is not installed as indicated.
2. Set time by turning the knob.
3. Insert one “AA“ (1.5V) battery as indicated in the battery holder for pendulum.
4. Gently swing the pendulum.

**Market supplier:**

**Jasněna Vláhová**

**Nové Město nad Metují**

[**www.vlahova.cz**](http://email.seznam.cz/redir?hashId=824343731&to=http://www.vlahova.cz)