**JVD quartz wall clock N20123**

1. Carefully unpack your clock.

2. Open the glass front.

3. Fold dial (Hold number 9 and open in the direction at home)

4. You will see two different spaces for the batteries: the back wall of watches for the melody, on the dial on the back for the hands and pendulum.

5. Insert the batteries.

6. Return the dial to its original position (close)

7. Hang up the clock and turn on the pendulum.

8. By turning the minute hand clockwise, set the time.

Caution: Do not turn the needles counterclockwise. In this case, the melody and the chime will not function properly.

9. Chime synchronization: Press the red button on the chime movement. With each press, the clock will sound once more. Press the button until you reach the desired number.

10. Selecting the melody: To select a melody, use a 4-position moving switch (mode):

Position 1: Melodies For Elise

Position 2: Chime every hour

Position 3: Melody Westminster with the chime every hour from 6:00 a.m. to 9:00 p.m.

Position 4: Melody Westminster

Chime volume can be adjusted by turning the wheel on the movement of melodies and chime.

11. Close the glass front.

12. Replace the batteries once a year, even if the clock still works. If the clock is no longer in use, remove the batteries to avoid possible damage.

Always use a soft cloth for cleaning. Never use abrasive materials or sand.