**JVD – RB8203 – user manual (EN)**

**Thank you so much for your choosing.**

This is a alarm clock which with Radio control function. Please open the battery cover (on the back side of clock ), to put two pcs of AAA battery in correct direction. Then put on the battery cover . now,



you will hear “BI”, then the clock is working. You will see wave symbol “ ” is flashing. It will search the signal automatically, about 5-10 minutes, it will collect the signal, and now the clock show the correct time.

**Name of each Button**

1. ALARM 2. SET 3. UP 4. DOWN 5. WAVE

6. SNOOZE /LIGHT (on the Top edge of clock )

Function:

1.display hour, minute, second, date, day, temperature（-9.9℃~~~~50℃）

2. calendar range : 2000—2099

3. day display: seven different language : GB, DE, FR, IT, ES, NL, DA

4. temperature : both ℃ & ℉ are available

5. With backlight touch sensor

6. with background light and snooze

7. With Radio control DCF

8. power : 2 PCS of AAA battery .

**How to set time**

1. Press “SET” more than 3 seconds, enter into set process.

A : “24Hr”is flashing, pres “UP” to choose 24Hr or 12Hr.

B: Press ”SET” again, ”00” is flashing, to set different time zones. You also can press ”SET” again to skip this setting(it’s not necessary progress)

C: Press “SET” again, ”hour” is flashing, to press “UP” or ”DOWN” to get what number you need.

D: Press “SET” again, ”minute” is flashing, to press “UP” or ”DOWN” to get what number you need.

E: Press ”SET” again, to set “YEAR”,”MONTH”,”DATE”,”DAY” in turn. Please note, there are seven different language of ”DAY”

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| language |  GB | DE | FR | IT | NL | ES | DA |
| DAY |  |  |  |  |  |  |  |

\*\*\*during setting process, if there is no any operation, will exit automatically, and the date is valid.

\*\*\*During setting process, if press “WAVE”, will exit automatically and open the Radio control function, to search the signal and display correct time

**How to set Alarm time**

1. Press “ALARM” for 3 second, “hour” is flashing, to press “UP” or ”DOWN” to get what number you need.
2. Press ”ALARM” again, to adjust “Minute” in turn
3. Press ”ALARM” again, to exit

\*\*\* under normal display, press ”ALARM” to see the alarm time,

\*\*\*under display alarm time, press ”UP” to open or close alarm.

\*\*\*the alarm lasts for 2 minutes. different period, the alarm sound will be different.

0-10 seconds, BI….BI…BI..BI…,

11—20 seconds, BIBI…BIBI…BIBI…BIBI…BIBI…BIBI,

21-30 seconds, BIBIBIBI…BIBIBIBI…,

after 30 seconds, BIBI, but sound quite hurry

\*\*\*during alarm time, press ”SNOOZE/LIGHT”, after 5 minutes, the alarm will be again, to press any other button, will close the alarm

**How to change ℃ & ℉**

 Under normal display , press ”DOWN” to choose ℃ or ℉

**Details about Radio control**

After you put the battery, it will search and receive the signal.

In this three point of time everyday, AM 1:00 ,2:00,3:00, t will search and the signal automatically.

If it does not receive the signal. it will search again at AM 4:00,if it’s fail, it will again at AM 5:00. If it’s still fail. Will start at next AM 1:00.

\*\*\* during the period of search signal, all the button is not available except SNOOZE/LIGHT & WAVE.

\*\*\* during the period of search signal, if the alarm ringing, it will exit search automatically.



\*\*\* during the period of search signal, this mark is flashing,after receive, it will display ,with full antenna sign

**How to do if it does not receive signal ?**

1. To press ”WAVE” to search and receive signal again.
2. To set the time according the above details “how to set the time”

**Special details**

1. Press “WAVE” more than 3 seconds, to open or close Radio control function.
2. When it’s DST period (Daylight Saving Time), you will see mark “S” ,near with the signal of

